# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of equipment for demining and destruction of unexploded ordnance p 1 /…**

**Publication reference:** NEAR/BEG/2023/EA-OP/0149

**LOT 2 – Supply of vehicle for the transport of unexploded ordnance**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

Unless otherwise specified, the requirements in these Technical Specifications are presented as a minimum standard which the offered goods must meet.

| **1.**  **No.** | **2.**  **Mandatory specifications** | **3.**  **Offered specifications** | **4.**  **Notes, remarks, reference to documents** | **5.**  **Notes of the evaluation committee** |
| --- | --- | --- | --- | --- |
| **1.** | **Armored off-road vehicle protection level according to European standard EN 1522/EN 1063, level No 6 or No 7**  **Quantity: 1 vehicle**  Note: for the safe and secure transportation of unexploded ordnance  **Required technical characteristics:**   * Equipped with diesel engine and air conditioning * 4 W drive * Off-road capability (off-road driving) * Maximum speed on the road ≥ 120 km / h * Wheel hub reductions, * Left hand drive, * Manual gearbox 6/1, * 1+2 seats with seat belts, * Drum brakes - pneumatically assisted, АBS. * Tires 14.00 Р 20 tubeless, * Clearance 380 mm, * Fuel tank: 220 or 320 liters, * Weight of empty vehicle: 12.000-16.000 kg, * Maximum load of explosive material: 150 kg * Equipment: * Battery: 170 Ah * Trailer hitch with automatic start of electric and brake couplings * Winch capacity 54 kN, rope length 30 m minimum, * Fire extinguisher, * Jack, spare tools and accessories for maintenance and repairs, * Wheel wrench * Anti-fragment explosion containment vessel. |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: “Kasarna Aerodrom”, Jabučki put bb, 26000 Pančevo, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Training** (upon delivery) on equipment handling (working with the equipment in all basic functions of the equipment), equipment maintenance.  Details of proposed training methodology, should be presented in the tender proposal and shall refer to the related equipment |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |