***ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

**Contract title: Procurement of Equipment for Plant Variety Testing p 1 / 7**

**Publication reference:** NEAR/BEG/2021/EA-OP/0081

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

Lot 3: Supply of portable computers for on-site data processing

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Portable computers for on-site data processing**  **Quantity: 11**  Minimum technical requirements:  - Screen 15.6” LED Full HD;  - Processor Type Average CPU Mark over 5200 on the PassMark CPU rating benchmarks ;  - RAM 8 GB (1 slot free);  - Disk 256 GB SDD;  - 64-bit native Operating System for personal computer featuring*:*  a) Customizable Graphical User Interface (GUI);  b) Package manager, capable to freely  obtain packages ad security updates;  c) The capability of authenticating to a  Microsoft Active Directory Domain Controller”.  - Graphics CardNvidia GeForce-MX110-2GB;  - 1 × HDMI;  - 1 × USB 3.0 (minimum);  - 1 x microphone, integrated;  - 1 x speakers;  - Wi-Fi Wireless network standards: IEEE 802.11a/b/g/n/ac;  - Bluetooth Wireless 3.0;  -Wired Communication Gigabit Ethernet LAN;  - Sound Audio supported 24-bit stereo format, integrated stereo speakers, integrated microphone;  - Battery Lithium-ion, 3 cells minimum;  - Integrated Camera 720p HD webcam (minimum);  - Compatible Laptop bag. |  |  |  |

|  |  |  |
| --- | --- | --- |
| **Commercial warranty** |  |  |
|  | Minimum 2 years (1 year after the end of 1 year standard warranty after provisional acceptance in accordance with the conditions laid down in Article 32 of the General Conditions) with free spare parts and authorised service technicians. Provide a link to the manufacturers web pages on which the user can verify the duration and type of warranty based on the serial number of the device. |  |
| **Response time and repair time** |  |  |
| **Response time** | * On-site response time within 24 hours from the date of the failure of equipment during 3 years after provisional acceptance. * Tenderer must provide a detailed description of the organisation of the proposed service (e.g. name of the authorised service provider). |  |
| **Repair time** | * 2 days repair time during 3 years after provisional acceptance. * Tenderer must provide a detailed description of the organisation of the proposed service (e.g. name of the authorised service provider). |  |
| **Delivery deadline** | 120 days from the date of conclusion of the contract. |  |

**Verification operations:**

**Installation:** The Contractor will be responsible for installation, configuration and start up of the equipment in accordance with the directions provided by the Beneficiary. The Beneficiary reserves the right to delegate one/two of its employees to activly participate in the installation and testing of the equipment together with the Contractors’s team.

**Testing:** Items shall be tested during the takeover event, where all the required specifications and features shall be accounted for, and full functionality of the items shall be presented.

**Annex 1**

**DISTRIBUTION LIST**

|  |  |  |
| --- | --- | --- |
| **Place and address of delivery/acceptance** | **Quantity** | **Name of the persons responsible for acceptance of the equipment and their full contact details (including phone number)** |
| **PSSS Sombor – Agricultural extension** **service Sombor**  Address: 35 Staparski put  25000 Sombor | 1 | Vladimir Sabadoš, Director  063541583 |
| **Faculty of Agriculture Novi Sad**  Trg Dositeja Obradoviča 8,  21101 Novi Sad  Serbia | 1 | Dragoslav Ivanišević, Professor  063557130 |
| **Faculty of Agriculture Belgrade**  Nemanjina 6,  11080 Belgrade (Zemun)  Serbia | 1 | Gordan Zec, Professor  0638601896 |
| **Fruit Research Institute, Čačak**  Kralja Petra I 9  32102 Čačak  Serbia | 2 | Ivana Glišić, DUS testing expert  0692402229  Žaklina Stajić Karaklajić, DUS testing expert  0641966397 |
| **Department for plant variety registration**  Plant Protection Directorate  Ministry of Agriculture, Forestry and Water Management  Omladinskih brigada 1, SIV 3,  11070 Novi Beograd  Serbia | 6 | Dragan Dedić, Chief of Department  0648235602  Dejan Vuković, Registration of agricultural species  0643150775  Katarina Zarubica, Registration of vegetable varieties  0641257528  Danijela Stojanović, Registration of oil crops  0605505068  Marina Vučković, Registration fodder plants and small grains  0642939607  Aleksandar Tabaković, Registration of fruit and vine varieties  0648055745 |